**Parking Sensor 4 Sensors 22mm LED Backlight Display Reverse Backup Radar Monitor System for vw saab bmw hyundai**

**Features:**

4 sensor system, double CPU and advanced chipset for enhanced coverage and detection (0-2m).  
With digital colored LED display (number & light).  
Help to prevent dangerous and costly collisions.  
Help to provide increased safety for passengers, pedestrians and family members who happen to be around the moving vehicle.  
Detect small children and low walls as well.  
Anti-freeze and rain proof.  
Easy to install.  
A saw drill head included.

**Specification:**

Type: Car parking radar

Material: Plastic

Quantity: 1pcs

Color: Black

Rate Voltage: 12V DC

Rate Operating Range: 9V - 16V DC

Rate Current: 20mA - 200mA

Detecting Distance: 0-2.5m / 0-8.2ft

Ultrasonic Frequency: 40KHz

Control Box Working Temperature: -30 - 80 celcius

Display Working Temperature: -20 - 70 celcius

Sensor Diameter: 22mm

LED Display Size: 9\*1.5cm / 3.5\*0.6"

Control Box Size: 9\*6\*2.2cm / 3.5\*2.4\*0.9"

Display Weight: 0.088kg / 3.1oz

**FAQ:**

1.No obstacle, have  BIBI sound

Answer: Red connect to turn lights, black connect  the whole car lights, do not connect the negative.

2. No obstacle,display other number   
  
(1) The display shows different numbers, such as E03-E07,

Answer:because the Electric current is not stable, buy a regulator specifically connected to the lights, do not shunt with the other   
  
(2) display same number    
Answer: Sensors should have 50 cm high, with the universal meter amount,sensors should be level, otherwise it will detect the ground.

https://ae01.alicdn.com/kf/HTB1NdwyKhWYBuNjy1zkq6xGGpXaM.jpg?width=960&height=50&hash=1010

1\*Main Control Box

1\*LED Display Indicator  
4\*Parking Sensors with 2.5M/8.2ft Line  
1\*Hole Saw  
1\*A saw drill head  
1\*Power Cable  
2\*Double Side Sticker